##

# Zebra Setup Utilities

## Build v1.1.9.1042

Welcome
Requirements
Supported Printers
Tips and Advice
Known Issues
Change Log
Getting Updates

### Welcome!

This Setup Utility makes it easy to configure Zebra printers. Six "Wizards" are available:

1. "Configure Printer Settings"
2. "Configure Print Quality"
3. "Configure Printer Connectivity"
4. "Download Fonts and Graphics"
5. "Printer Tools"
6. "Open Communication with Printer"

All Wizards use installed ZebraDesigner drivers to interact with printers.
Back to Top

### 1. Requirements

This software is supported on 32-bit and 64-bit Microsoft Windows XP, Windows 2003, Windows 2008, Windows Vista® and Windows 7.
Windows is a registered trademark of Microsoft Corporation in the United States and other countries.
Back to Top

### 2. Supported Printers

The following Zebra printers are supported in this version:
105SL 203DPI
105SL 300DPI
110PAX3 203DPI
110PAX3 300DPI
110PAX3 600DPI
110PAX4 203DPI
110PAX4 300DPI
110Xi4 203 dpi
110Xi4 300 dpi
110Xi4 600 dpi
110XiIII Plus 200DPI
110XiIII Plus 300DPI
110XiIII Plus 600DPI
140Xi4 203 dpi
140XiIII
140XiIII Plus
170PAX3 203DPI
170PAX3 300DPI
170PAX4 203DPI
170PAX4 300DPI
170Xi4 203 dpi
170Xi4 300 dpi
170XiIII
170XiIII Plus
170XiIII Plus 200DPI
220Xi4 203 dpi
220Xi4 300 dpi
220XiIII
220XiIII Plus
220XiIII Plus 300DPI
2746e
888-DT
888-TT
90XiIII
90XiIII Plus
96XiIII
96XiIII Plus
DA402
EZ 320
GK420d
GK420d (EPL)
GK420t
GK420t (EPL)
GC420d
GC420d (EPL)
GC420t
GC420t (EPL)
GK888d
GK888d (EPL)
GK888t
GK888t (EPL)
GT800 (EPL)
GT800 (ZPL)
GX420d
GX420d (EPL)
GX420t
GX420t (EPL)
GX420s
GX420s (EPL)
GX430t
GX430t (EPL)
HC100 300 dpi
KR403
LP 2824
LP 2824 Plus (EPL)
LP 2824 Plus (ZPL)
LP 2824-Z
LP 2844
LP 2844-Z
Mobile Printer
MZ 220
MZ 320
P4T (CPCL)
P4T (ZPL)
QL 220/QL 220 Plus
QL 320/QL 320 Plus
QL 420/QL 420 Plus
QLn220
QLn320
QLn220 (ZPL)
QLn320 (ZPL)
R-402
ZE500-4 LH-203dpi ZPL
ZE500-4 LH-300dpi ZPL
ZE500-4 RH-203dpi ZPL
ZE500-4 RH-300dpi ZPL
ZE500-6 LH-203dpi ZPL
ZE500-6 LH-300dpi ZPL
ZE500-6 RH-203dpi ZPL
ZE500-6 RH-300dpi ZPL
R110PAX4 LH-203DPI
R110PAX4 LH-300DPI
R110PAX4 RH-203DPI
R110PAX4 RH-300DPI
R110Xi 200DPI
R110Xi 300DPI
R110Xi HF 200DPI
R110Xi HF 300DPI
R110Xi4 203 dpi
R110Xi4 300 dpi
R110Xi4 600 dpi
R110XiIII Plus
R170Xi 200DPI
R170Xi 300DPI
R2844-Z
R4Mplus
RP4T (ZPL)
RW 220
RW 420
RW4-PS
RZ400 200 dpi
RZ400 300 dpi
RZ600 200 dpi
RZ600 300 dpi
S400
S4M-203dpi EPL
S4M-203dpi ZPL
S4M-300dpi ZPL
ZT210-200dpi ZPL
ZT210-200dpi EPL
ZT210-300dpi ZPL
ZT220-200dpi ZPL
ZT220-200dpi EPL
ZT220-300dpi ZPL
ZT230-200dpi ZPL
ZT230-200dpi EPL
ZT230-300dpi ZPL
S600
T402
TLP 2824
TLP 2824 Plus (EPL)
TLP 2824 Plus (ZPL)
TLP 2824-Z
TLP 2844
TLP 2844-Z
TLP 3842
TLP 3844-Z
Z4M 203DPI
Z4M 300DPI
Z4Mplus 203DPI
Z4Mplus 300DPI
Z6M 203DPI
Z6M 300DPI
Z6Mplus 203DPI
Z6Mplus 300DPI
ZM400 200 dpi (EPL)
ZM400 200 dpi (ZPL)
ZM400 300 dpi (ZPL)
ZM400 600 dpi (ZPL)
ZM600 200 dpi (EPL)
ZM600 200 dpi (ZPL)
ZM600 300 dpi (ZPL)
Back to Top

### 3. Tips and Advice

Windows Vista and Windows 7 have enhanced control over permissions. When installing in these operating systems, it is recommended that an Administrator account be used.
The Status Monitor regularly checks the printer for current status information. When the driver is being used over a network connection, this can have the effect of consuming connection ports that would otherwise be used for accepting print jobs at the printer. If the Status Monitor is in use and you are experiencing a delay in printing, try right clicking over the Status Monitor in the system tray (by the clock) and closing the Status Monitor.
Back to Top

### 4. Known Issues

When using a printer and Bluetooth communication with the Setup Utility or the Status Monitor, continuous disconnecting/connecting and prompting for credentials will occur if simple secure pairing is used.
Back to Top

### 5. Change Log

V1.1.2.790 | 02/09/2011 | Added support for Mobile printers.
V1.1.2.838 | 07/06/2011 | For mobile printers, commands for print speed, darkness and media type are now sent to the printer and/or saved to a file. The direct communication window can now receive all data sent by the printer. A port polling time out option can be adjusted to control this. For mobile printers, there is now a ‘send and store’ file option in the printer tools wizard. The PEAP, EAP-FAST, EAP-TLS and EAP-TTLS wireless securities are now enabled correctly. Corrected translations in various languages. The darkness wizard now prints the entire batch of labels using the correct darkness settings. The connectivity wizard button is now enabled when selecting the KR403 printer. For EPL printers, the linerless media option command is now sent when selected in the printer settings wizard. The Bluetooth friendly name is not sent to the printer if the Bluetooth enabled option is unchecked. For QLn printers the correct commands are now sent to set static ip addresses. For QLn printers commands are now generated for the wired network option.
V1.1.3.838 | 8/15/2011 | The "Send and store file in printer memory" feature for Mobile printers has been corrected. The GX420s is now supported. Added Bluetooth Minimum Security Mode option in connectivity wizard for EZ and QLn mobile printers.
V1.1.4.838 | 9/14/2011 | The "Send and Store" feature for Mobile printers has been corrected.
V1.1.8.986 | 1/20/2012 | Added the ability to set communication timeout in the options dialog. Added the ability to select Standard or Internal character delimiters in the options dialog. Added the ability to set the printer DNS name in the connectivity wizard. "Connecting to printer" status message is now cleared in the direct comm window once communication is established with the printer. Username field is now enabled for EAP-TLS. The output is now correct when using three certificate files. Bluetooth friendly name is not changed if no name is entered. A dash character can now be used in the Bluetooth friendly name. Binary data can now be received and displayed in the direct comm window. Sensor settings can be set in the Printer Settings Wizard for ZPL printers. Corrected SGD command output for Wired interface settings. Corrected some translations. Time interval setting in Printer Settings Wizard is now enabled for mobile printers. 802.11n radio settings are available for ZT and QLn printers. Connectivity Wizard is now enabled for Tabletop printers with EPL firmware. The following printer models are now supported. GC420d GC420d (EPL) GC420t GC420t (EPL) QLn220 (ZPL) QLn320 (ZPL) ZE500-4 LH-203dpi ZPL ZE500-4 LH-300dpi ZPL ZE500-4 RH-203dpi ZPL ZE500-4 RH-300dpi ZPL ZE500-6 LH-203dpi ZPL ZE500-6 LH-300dpi ZPL ZE500-6 RH-203dpi ZPL ZE500-6 RH-300dpi ZPL ZT210-200dpi ZPL ZT210-200dpi EPL ZT210-300dpi ZPL ZT220-200dpi ZPL ZT220-200dpi EPL ZT220-300dpi ZPL ZT230-200dpi ZPL ZT230-200dpi EPL ZT230-300dpi ZPL
V1.1.9.1042 | 3/14/2012 | Corrected an issue with the "Open Communication with Printer" window minimizing in Vista and Windows 7. Corrected some translations. Implemented the ability to configure 802.11n settings on applicable printers. Updated the sensor settings dialog in the Configure Printer Settings wizard.

Back to Top

### 6. Getting Updates

The Zebra Setup Utility is frequently updated and modified to take advantage of new developments. Updated versions will be available on our web site: http://www.zebra.com/setup
Back to Top
Zebra Technologies Corporation (C) 2012 ZIH Corp. All rights reserved.